# Air ULD Container

Container, Cooltainer and Pallet

### Air ULD Container

### LD- 3 Container
IATA RATE CLASSIFICATION | 8-CONTOUR No. E
IATA ID CODE | AVE/AKE
DIMENSION (Inch) | L-79/61.5 x W-60.4 x H-64
LOAD CAPACITY (kg/lbs.) | 1,587-1,588/3,890
VOLUME (cu.m.) | 4.3 m3
TARE WEIGHT (kg/lbs.) | 82-92/225
LOADING POSSIBILITY | 747,777,MD11,D10.L10, A300,A310,A330,A340,AB6
### LD- 3 Container
IATA RATE CLASSIFICATION | 8-CONTOUR No. N
IATA ID CODE | RKN
DIMENSION (Inch) | L-79/61.5 x W-60.4 x H-64
LOAD CAPACITY (kg/lbs.) | 1,587-1,588/3,890
VOLUME (cu.m.) | 3.7 m3
TARE WEIGHT (kg/lbs.) | 190/466
LOADING POSSIBILITY | 747,777,MD11,D10.L10, A300,A310,A330,A340,AB6
### 88" x 125" Pallet
IATA RATE CLASSIFICATION | 5
IATA ID CODE | PAG,PAJ,PAU,PAP,P1P,PAW
DIMENSION (Inch) | 88 x 125
LOAD CAPACITY (kg/lbs.) | 6,033/14,781
VOLUME (cu.m.) |
TARE WEIGHT (kg/lbs.) | 96-110/270
LOADING POSSIBILITY | 747,777,MD11,D10.L10, A300,A310,A330,A340,AB6
### 96" x 125" Pallet
IATA RATE CLASSIFICATION | 28G
IATA ID CODE | PMC
DIMENSION (Inch) | 96 x 125
LOAD CAPACITY (kg/lbs.) | 6,804/16,670
VOLUME (cu.m.) |
TARE WEIGHT (kg/lbs.) | 113-118/289
LOADING POSSIBILITY | 747,74F,777,A300,A310 A330,A340,AB6
### LD- 9 Container
IATA RATE CLASSIFICATION | 5-CONTOUR No. P
IATA ID CODE | AAP
DIMENSION (Inch) | L-125 x W-88 x H-64
LOAD CAPACITY (kg/lbs.) | 6,033/14,781
VOLUME (cu.m.) | 10.3-10.6 m3
TARE WEIGHT (kg/lbs.) | 200-204/4998
LOADING POSSIBILITY | 747,74F,777,MD11,D10,D10F, L10,A300,A310,A330,A340,AB
### LD-9 Cooltainer
IATA RATE CLASSIFICATION | 5-CONTOUR No. P
IATA ID CODE | RAP
DIMENSION (Inch) | L-125 x W-88 x H-64
LOAD CAPACITY (kg/lbs.) | 6,033/14,781
VOLUME (cu.m.) | 9.7 m3
TARE WEIGHT (kg/lbs.) | 355/870
LOADING POSSIBILITY | 747,74F,777,MD11,D10,D10F, L10,A300,A310,A330,A340,AB6
### LD- 6 Container
IATA RATE CLASSIFICATION | 6-CONTOUR No. F
IATA ID CODE | ALF
DIMENSION (Inch) | L-160/125 x W-60.4 x H-64
LOAD CAPACITY (kg/lbs.) | 3,175/7,779
VOLUME (cu.m.) | 8.9-9.2 m3
TARE WEIGHT (kg/lbs.) | 152-186/456
LOADING POSSIBILITY | 747,777,MD11,D10,L10, A300,A310,A330,A340,AB6
### LD- 26 Container
IATA RATE CLASSIFICATION | 5-CONTOUR No. F
IATA ID CODE | AAF
DIMENSION (Inch) | L-160/125 x W-88 x H-64
LOAD CAPACITY (kg/lbs.) | 6,033/14,781
VOLUME (cu.m.) | 13.1-14.5 m3
TARE WEIGHT (kg/lbs.) | 250/613
LOADING POSSIBILITY | 747,777,MD11,D10,L10, A300, A310,A330,A340,AB6
### LD- 36 Container
IATA RATE CLASSIFICATION | 2BG-CONTOUR No. F
IATA ID CODE | AMF
DIMENSION (Inch) | L-160/125 x W-96 x H-64
LOAD CAPACITY (kg/lbs.) | 6,804/15,000
VOLUME (cu.m.) | 14.7 m3
TARE WEIGHT (kg/lbs.) | 290
LOADING POSSIBILITY | 747, 777, L10, A300,A310, A330, A340, AB6
### 60.4" x 125" Pallet
IATA RATE CLASSIFICATION | 6
IATA ID CODE | PLA
DIMENSION (Inch) | 60.4 x 125
LOAD CAPACITY (kg/lbs.) | 3,175/7,779
VOLUME (cu.m.) |
TARE WEIGHT (kg/lbs.) | 101-104/255
LOADING POSSIBILITY | 747,777,MD11,D10,L10,A300, A310,A330,A340,AB6
### 96" x 238.5 Pallet
IATA RATE CLASSIFICATION | 1
IATA ID CODE | PGA
DIMENSION (Inch) | 96 x 238.5
LOAD CAPACITY (kg/lbs.) | 13,608-30,000/73,500
VOLUME (cu.m.) | 14.7 m3
TARE WEIGHT (kg/lbs.) | 486/1,191
LOADING POSSIBILITY | 74F,D10F,A300C,A310C