# Ocean Freight Container

Dry Container, Refrigerated Container, Open Top Container and Flat Rack Container

### Ocean Freight Container

### Dry Container Display the table in ft/lbs
Dry / Steel | Door openings (mm) | Internal dimensions(mm) | Weight (kg) | Volume (m3)
Type | Size | Width | Height | Length | Width | Height to load line | Max. Gross | Tare | Max. Payload | Capacity to load line
20" std | 20' x 8' x 8' 6" | 2,340 | 2,274 | 5,896 | 2,350 | 2,385 | 27,000 | 2,150 | 24,850 | 33
40" std | 40' x 8' x 8' 6" | 2,339 | 2,274 | 12,035 | 2,350 | 2,393 | 32,500 | 3,700 | 28,800 | 67
40" high | 40' x 8' x 9' 6" | 2,340 | 2,577 | 12,035 | 2,350 | 2,697 | 34,000 | 3,800 | 30,200 | 76
45" high | 45' x 8' x 9' 6" | 2,340 | 2,585 | 13,556 | 2,352 | 2,697 | 32,500 | 4,800 | 27,820 | 86
Dry / Aluminium | Door openings (mm) | Internal dimensions (mm) | Weight (kg) | Volume (m3)
Type | Size | Width | Height | Length | Width | Height to load line | Max. Gross | Tare | Max. Payload | Capacity to load line
40" wide door | 40' x 8' x 8' 6" | 2,343 | 2,278 | 12,056 | 2,347 | 2,379 | 32,500 | 2,790 | 29,710 | 67
40" high | 40' x 8' x 9' 6" | 2,343 | 2,584 | 12,056 | 2,347 | 2,684 | 32,500 | 2,900 | 29,600 | 76
45" high | 45' x 8' x 9' 6" | 2,340 | 2,584 | 13,582 | 2,347 | 2,696 | 32,500 | 3,900 | 28,600 | 86
### Refrigerated Container
Reefer / Steel | Door openings (mm) | Internal dimensions (mm) | Weight (kg) | Volume (m3)
Type | Size | Width | Height | Length | Width | Height to load line | Max. Gross | Tare | Max. Payload | Capacity to load line
20" std | 20' x 8' x 8' 6" | 2,294 | 2,201 | 5,451 | 2,290 | 2,156 | 30,480 | 2,930 | 27,550 | 27,9
40" high | 40' x 8' x 9' 6" | 2,278 | 2,473 | 11,578 | 2,280 | 2,425 | 34,000 | 4,500 | 29,500 | 64
Reefer / Aluminium | Door openings (mm) | Internal dimensions (mm) | Weight (kg) | Volume (m3)
Type | Size | Width | Height | Length | Width | Height to load line | Max. Gross | Tare | Max. Payload | Capacity to load line
20" std | 20' x 8' x 8' 6" | 2,286 | 2,188 | 5,430 | 2,286 | 2,155 | 27,000 | 2,750 | 24,250 | 26,8
40" std | 40' x 8' x 8' 6" | 2,294 | 2,174 | 11,577 | 2,294 | 2,110 | 32,500 | 3,900 | 28,600 | 56,1
40" high | "40' x 8' x 9' 6" | 2,290 | 2,535 | 11,577 | 2,294 | 2,409 | 32,500 | 4,150 | 28,350 | 64,1
### Open Top Container
Open-tops / Steel | Internal dimensions (mm) | Door openings (mm) | Top openings (mm) | Weight (kg) | Volume (m3)
Type | Size | Length | Width | Height | Width | Height | Length | Width | Max. Gross | Tare | Max. Payload | Capacity
20' open-top | 20'x 8'x 8'6" | 5,919 | 2,340 | 2,286 | 2,286 | 2,251 | 5,425 | 2,223 | 24,000 | 2,177 | 28,230 | 32
40' open-top | 40'x 8'x 8'6" | 12,043 | 2,338 | 2,272 | 2,289 | 2,253 | 11,622 | 2,162 | 30,480 | 4,300 | 28,700 | 64
Open-tops / Aluminium | Internal dimensions (mm) | Door openings (mm) | Top openings (mm) | Weight (kg) | Volume (m3)
Type | Size | Length | Width | Height | Width | Height | Length | Width | Max. Gross | Tare | Max. Payload | Capacity
20' open-top | 20'x 8'x 8'6" | 5,893 | 2,346 | 2,353 | 2,338 | 2,273 | 5,488 | 2,230 | 30,480 | 2,250 | 21,823 | 32
### Flat Rack Container
Flat rack / Steel | Internal dimensions (mm) | Weight (kg)
Type | Size | Length | Width | Height | lenght between headers | lenght between corner posts | width between corner posts | Gross | Tare | Max. Payload
20' fixed-corner | 20' x 8" x 8" 6" | 5,935 | 2,398 | 2,327 | 5,935 | 5,693 | 2,106 | 24,000 | 2,560 | 21,440
20' collapsible | 20' x 8' x 8' 6" | 5,966 | 2,418 | 2,286 | 5,850 | 5,422 | 2,058 | 30,480 | 2,970 | 27,510
40' fixed-corner | 40' x 8' x 8' 6" | 12,080 | 2,438 | 2,103 | 12,080 | 11,796 | 2,114 | 30,480 | 5,480 | 25,000
Flat rack / Steel | Internal dimensions (mm) | Maximum load (kg) | Weight (kg)
Type | Size | Length | Width | Concentrated (kg/sq.feet) | on mid 10 ft | Max. Gross | Tare | Max. pay load
40 atd | 40'x 8'x 20' 3/8" | 12,052 | 2,438 | 4,535 | 12,148 | 44,440 | 4,860 | 39,580
Please note there may be slight size variations for some containers, as well as limitations regarding acceptance in certain locations.